|  |  |
| --- | --- |
| Blade size | 0.6 x 3.5 mm |
| Clamping range, max. | 4 mm² |
| Clamping range, min. | 0.13 mm² |
| Clamping screw | M 2.5 |
| Connection cross-section, stranded, max. | 4 mm² |
| Connection cross-section, stranded, min. | 0.5 mm² |
| Connection direction | on side |
| Gauge to IEC 60947-1 | A3 |
| Number of connections | 7  |
| Stripping length | 8 mm |
| Tightening torque, max. | 0.6 Nm |
| Tightening torque, min. | 0.4 Nm |
| Type of connection | Screw connection |
| Wire connection cross section, finely stranded, max. | 4 mm² |
| Wire connection cross-section, finely stranded with wire-end ferrules DIN 46228/1, max. | 2.5 mm² |
| Wire connection cross-section, finely stranded with wire-end ferrules DIN 46228/1, min. | 0.5 mm² |
| Wire connection cross-section, finely stranded with wire-end ferrules DIN 46228/4, max. | 2.5 mm² |
| Wire connection cross-section, finely stranded with wire-end ferrules DIN 46228/4, min. | 0.5 mm² |
| Wire connection cross-section, finely stranded, min. | 0.5 mm² |
| Wire connection cross-section, solid core, max. | 4 mm² |
| Wire connection cross-section, solid core, min. | 0.5 mm² |