**Product Details**

3M™ Double Coated Foam Tape 9515W is a white, 1.5mm thick, double coated polyethylene foam tape with acrylic adhesive.

The acrylic adhesive provides good initial tack and adhesion to a wide variety of surfaces.

* White, 1.5 mm thick, closed-cell double coated polyethylene foam with acrylic adhesive
* Mount and join a wide range of materials

**Specifications**

|  |  |
| --- | --- |
| **Adhesive Type** | **Acrylate** |
| **Backing Material** | **Polyethylene** |
| **Industries** | **Metalworking, Signage, Transportation** |
| **NPVI Mktg** | **Nē** |
| **Overall Length (Metric)** | **33 m** |
| **Overall Width (Metric)** | **19 mm** |